picprojects.org.uk/projects/zcode/
rgbtest.exe


Copy all files in to a new subdirectory.

rgbtest.exe /? will show command line options

rgbtest.exe will run test using COM1 @ 9600bps

The test sends a series of colour data / transfer commands
to the broadcast address lasting approximatley 30 seconds

Use this application to test newly built driver hardware.

Since data is sent to the broadcast address, as long as the 
correct  Comm port and bit rate are used all drivers on the
bus should display changing colours.

rgbtest.pl is the perl source code for the application






